| Contents

[Main setting] tab Switching between color print and monochrome print, paper type, output method, etc. can be set. Output image Shows output image according to current settings. Color mode Selects color or monochrome printing. Original image Selects image or character to which priority is given in printing. Duplex printing Selects whether or not to perform duplex printing. To select the duplex printing, specify the binding position.
[Settings]
- | OFF | Duplex printing is not performed.
- | Long edge binding | Duplex printing is performed. The long edge of the original becomes the binding position.
- | Short edge binding | Duplex printing is performed. The short edge of the original becomes the binding position.
Paper feed tray Selects the feed tray in which paper to be used for printing is set.
[Settings]
- | Auto tray selection | The feed tray is automatically selected according to the settings of [Paper type] on the [Main setting] tab and [Output Paper size] on the [Layout] tab.
Note: | When there is no tray whose conditions correspond on the printer, an error occurred and the data cannot be printed.
- | Feed Tray 1 | Printing is performed onto the paper set in Feed Tray 1.
- | Feed Tray 2 | Printing is performed onto the paper set in Feed Tray 2.
- | Standard Feed Tray | Printing is performed onto the paper set in the Standard Feed Tray.
Paper type Selects the paper type. Ejection mode Selects whether to perform collated printing or non collated printing. Pause after proof Sets whether or not to output proof copy. If you click [Pause after proof] to display a checkmark, you can check the print by printing only one page or one set first (not included in the specified number of copies). After checking, if no problem is found, press the PRINT/PAUSE key on the printer to continue printing. It is useful when printing a lot of pages or printing a lot of copies. Output mode Selects the output mode of data sent from the computer.
[Settings]
- | Direct print | Prints data immediately onto paper transmitted from a computer.
- | Print and Storage | Performs direct printing and also stores the output data in the printer controller (Storage).
- | Archive | Store printing data with RIP status.
- | Storage | Stores the output data in the printer controller. Data kept in storage can be printed repeatedly.
Specify output condition The output conditions of Printer Driver that have been registered in the printer controller can be selected. In addition, the storage folder for output data in storage can be specified, the folder security code and the job comment can be input.
[Settings]
- | Output condition | A registered output condition can be selected if [Output mode] is set to [Direct print] and [Print & Storage].
- | Storage folder name | The storage folder for output data in storage can be selected, if [Output mode] is set to [Print & Storage] and [ Storage].
- | Folder Security code | The folder security code is required, when storing the data in the folder that is set the security code.
- | Job comment | The comment input here can be displayed on the [Detail] screen under the [Job manager].
Default Returns the settings on the [Main setting] tab to the default settings. Help Displays Help.