PS7R-9000/5000 Help

| Contents

[Options] tab

Sets the method of job separation, print density, clustering and security print.

Job separation
Inserts job separation paper between jobs or between sets or pages when printing multiple jobs or copies. Sets the feed tray used for job separation paper on the Operation Panel of the printer in advance.

[Settings]
- | OFF | Job separation is not performed.
- | Between jobs | Job separation paper is automatically inserted between jobs.
- | Every division | Inserts automatically separation paper each time a unit of collated printing or non collated printing is complete. Set collate or non collate at [Ejection mode] on the [Main setting] tab.

Print density
Adjusts the print density.

Clustering
When printing a lot of jobs or printing a lot of copies or a lot of pages, you can improve the efficiency of printer processing by splitting a job or distributing jobs to the linked printer controller on the network. Click the [Details] button to display the [Clustering] window. The linked printer controllers should be the same models.

Details
Click [Clustering] to display a check mark and click the [Details] button. Click the [Details] button to display the [Clustering] window.

[Settings]
- | Job delegation | If multiple units of HC5500 and PS7R (controller) are connected on the network , jobs can be distributed to these printers. If Job delegation is set to ON, when a new job is received while a job is being processed, the new job is sent for printing to a controller that has the highest priority is the order of the registered printer controller IP list and which exists actually.

-

Job split

When processing a job with a lot of pages or a lot of copies, you can split the job into multiple jobs. Load applied to the printer controller per job is reduced.
- Output-range-based Set the page number that triggers job split at [Job split limit].
- Print-volume-based Set the number of copies that triggers job split at [Job split limit].

- | Job split limit | Specifies the condition for job split. If the specified number of pages or copies is exceeded, job split is activated.

Security Print
When you output the document which does not want to be seen by other person, use the "Security Print". The Security code can be added to the output data.

[Settings]
- | Security code | The Security code can be input.The number can be input to 8 from 0 figures. The input of the security code is necessary when the job that is added a security code is operated from Job Manager.
- | Job name is not indicated on Job Manager. | If a check mark is attached, a job name is not displayed in the "Job Status" of Job Manager.