Printer Driver Help

| To Table of Contents

[Option settings] tab

Job separation, Print density, Clustering etc. are set.

Sorter Control (1-colour printers only)
When you have installed and are using a sorter (option) on the printer, sorter operations can be set. The sorter operates as follows according to each of the items selected in the pull-down menu.

[Items that can be set]
- | Open | Follows the settings on your RISO printer.
- | OFF | The sorter is not used.
- | Sort | Separate by page, and output each printout to a different bin. When the total number of pages for a job exceeds the number of bins in the sorter, the ones that exceed the number are output to the unsorted tray.
- | Group | Collect in groups, and output the printouts to different bins. Printouts of the same page are output to one bin.
- | Stack | When you want to have sufficient drying time for each printout, select this. When the total number of pages for a job exceeds the number of bins in the sorter, it starts again from the first bin and outputs in order.

Stapler(1-colour printers only)
If a sorter (option) equipped with a stapler is installed and used, you can set whether or not to stable the printouts and set the stapling position for the printouts.

[Selectable items]
- | Open | Follows the settings on your RISO printer.
- | OFF | The sorter does not operate.
- | Front 1 position |
- | Centre 2 positions |
- | Depth 1 position |

Job separation
The tape introduction timing can be set with a Job separator connected to the printer.

[Selectable items]
- | Open | Follows printer settings.
- | OFF | No tape insertion.
- | Between jobs | Tape is inserted between jobs.
- | Between Pages | Tape is inserted between pages.

Paper Interposal mode (front paper supply units only)
During printing, a sheet of paper different from the paper for printing can be inserted as a separator. The insertion timing interposed paper is set here. The tray used for the interposal paper must be set in advance.

[Selectable items]
- | Open | Follows printer settings.
- | OFF | No interposal paper.
- | Between jobs | Interposal paper is inserted between jobs.
- | Between Pages | Interposal paper is inserted between pages.

Print Speed
The printer print speed is adjusted in five gradations. When [Open] is selected, printing is done with the printer settings.

Print Density-Colour 1/Print Density-Colour 2
The printer print density is adjusted in five gradations. When [Open] is selected, print jobs are printed with the printer setting for density.

Start confidential operation at the end
After making a master and printing for all pages, the master created is discarded at the end and an new master is set up. When you do not want the next user of the printer to know the content printed, this should be set.

Output data after initializing printer
The printer settings are reset before the document data is sent to the printer. Basically, it is recommended that you have this checked.

High speed
The RISO printer prints at high speed. The speed will vary according to the RISO printer.

Interval printing
An interval for outputting paper is opened by interposing empty turns of the drum during printing, and it makes it easier to avoid offsetting the printing paper.

Clustering
This is splitting a job and distributing the job to other printer controllers on the network, so printer processing can be more efficient.

Details
This is available only when [Clustering] has been checked. Clicking it displays the [Clustering] window.

[Contents that can be set]
- | Job delegation | When multiple RISO PS7R Controllers are connected to the network, each of them can carry out job delegation. When Job delegation is ON and a new job is received while one job is being processed, the list of registered controllers is searched in order, and the new job is sent to be printed to a RISO PS7R Controller that is present.
- | Job split | When jobs with large numbers of pages or a large number of copies are being processed, the one job can be split into multiple jobs. The printer load for each job is reduced.
- | Job split limit | The conditions for splitting the job are set. If jobs exceeding the number of pages or number of copies specified here are printed, they are split.

Default
Resets the settings on the [Option settings] tab to their initial values.

Help
Displays Help.