Printer Driver Help

| To Table of Contents

[Main setting] tab

Mono-colour printing and dual-colour printing can be switched, and the output mode, etc., can be set.

Preview display
Allows you to view an image of the settings you make.

Colour mode(dual-colour printers only)
Select dual-colour or mono-colour printing.

Layout
When finishing for the printing is duplex printing, the binding side can be selected.

[Contents that can be set]
- | OFF (default) | No settings for duplex printing.
- | Long edge binding | The long edge of the original is selected for binding.
- | Short edge binding | The short edge of the original is selected for binding.

Paper feed tray (Multi tray paper feeder only)
Select the tray holding the paper for printing.

[Contents that can be set]

-

Auto tray selection

The tray is automatically selected according to the [Output paper size] on [Layout] tab.

When no tray matches the output paper size, it generates an error and printing cannot be carried out.

- | Feed Tray 1 | The paper in Tray 1 is used for printing.
- | Feed Tray 2 | The paper in Tray 2 is used for printing.
- | Standard Feed Tray | The paper in the Standard Feed Tray is used for printing.
- | Open | Regardless of the [Output paper size] set on the [Layout] tab, printing is done on the paper in the tray set by printer panel operations.

Specify print side
When the binding edge is set under [Layout], select whether the front side is printed or the back is printed.

[Contents that can be set]
- | Front page | Only odd numbered pages are printed.
- | Back page | Only even numbered pages are printed.

Auto process
Sets the continuous mode for master making and printing (print pause timing).

[Contents that can be set]
- | ON | Continuous operation from making a master to printing. When there are multiple pages, all pages are printed without stopping.
- | Semi-Auto (Print) | Stops after receiving the data and before making a master. The paper can be rearranged or the print drum replaced. Pressing the [Start] button on the RISO printer begins making a master and printing (Auto print).
- | Semi-Auto (Master) | After making a master, one test print is output and the process pauses. After checking the printout, you can adjust the position or make other adjustments. Pressing the [Start] button on the RISO printer begins the printing (Auto master). When there are multiple pages, the master for the next page is made (Auto master), and the process pauses after a test print is output.
- | Manual | Printing pauses before making a master and before printing. (This is the normal printing mode (manual).)

Output mode
Selects the output mode for the date sent from the computer.

[Contents that can be set]
- | Direct print | The data sent from the computer is printed on paper according to the [Auto process] settings.
- | Print & Storage | Along with direct printing, the output data is stored in the controller.
- | Storage | The output data is stored in the controller. Data stored in the storage can be reprinted or have the print output conditions changed by selecting the [Storage] tab under the RISO PS7R Console [Job manager].
- | Archive | The output data is stored (archived) after RIP. The stored data can be reprinted by selecting [Archive] under the RISO PS7R Console [Job manager].

Specify output condition
When something other than [Forms] is selected in [Output mode], the print settings that have been registered can be selected. In addition, the storage folder for output data in storage can be specified. Click the [Specify output condition] button to display its screen.

[Selectable items]
- | Output condition | You can select between printing according to the printer driver settings or printing with the output settings registered in the controller.
- | Storage folder | Output data can be stored in any folder created in the controller. When a folder is created in the controller with [Print & Storage] under [Output mode] or [Storage] selected, one for the folders, Folder 1 - Folder 9 (or any folder that has been set up), is selected.

Default
Resets the settings on the [Main setting] to their initial values.

Help
Displays Help.