| Contents

[Layout] tab Set the enlargement/reduction ratio in printing and the method of pagination. Output image Shows output image according to current settings. Original size Select the paper size specified with the application software. If the original size is different from the application setting, the setting in the application software takes precedence. Output paper size Select the paper size for printing. If the original size is different from the output paper size, enlargement/reduction is automatically performed according to the output paper size. Zoom Sets the image enlargement/reduction ratio for printing.
1. | Click [Zoom] to display a check mark.
2. | Click or to specify the enlargement/reduction ratio for printing in %.
Orientation Selects the orientation of original for printing. Pagination Selects the type of pagination.
[Settings]
- | OFF | Pagination is not performed.
- | Multi-up ( Single page) | A multiple number of same page are paginated onto a sheet.
- | Multi-up ( Multi-page) | A multiple number of continuous pages are paginated onto a sheet in the page order.
- | Booklet | A multiple number of continuous pages are paginated and printed so that a booklet can be obtained by binding at the centre. Two pages are printed on each side of paper.
- | Fold | A multiple number of continuous pages are paginated and printed so that a book can be obtained by folding in two (crosswise) after duplex printing, binding, and cutting. Four pages are printed onto each side of a sheet.
Pages per sheet Selects the number of pages per sheet for pagination. Selectable "pages per sheet" depends on the pagination.
[Settings]
- | Multi-up(Single page) | 2,4,8,16pages/sheet
- | Multi-up(Multi-page) | 2,4,8,16pages/sheet
- | Booklet | Need not be selected. (The number is automatically set to 2pages/sheet.)
- | Fold | Need not be selected. (The number is automatically set to 4pages/sheet.)
Page order Selects the order of arrangement of pages for pagination. If [Reverse order (from right to left)] is not checked, the direction is left to right, and if checked, the direction is right to left. Selectable "Page order" depends on the pagination.
[Settings]
- | Multi-up (Single page) | No
- | Multi-up (Multi-page) | Vertical/horizontal, reverse direction (from right to left)
- | Booklet | Reverse order (from right to left.)
- | Fold | Reverse order (from right to left.)
Reverse order (from right to left) Specifies whether it arranges on the left from the right. For [Booklet] and [Fold], when there is no checkmark, it is arranged for the left side binding and when there is a checkmark, it is for the right side binding. Output face Select the print sequence. (It specifies the printing surface up or down.)
[Settings]
- | Auto | The printer automatically outputs the data by the optimum print sequence (face up with descending or face down with ascending). It depends on the current settings.
- | Face down | Outputs printed paper with the printed face down. When two or more jobs are printed continuously, the printed documents are ejected in same order which received data.
Default Returns the settings on the [Layout] tab to the default settings. Help Displays Help.