| Contents

[Forms] tab A form registered in the printer controller can be selected for overlaying it on the output data for printing. Form print pattern Selects whether a form is printed onto the same face as output data (Single side overlay) or onto the reverse side( Double side overlay.)
[Settings]
- | OFF | No form is printed.
- | Single side overlay | A form is printed onto the same face as the output data. When carrying out duplex printing by the "Specify Front and Back respectively" can be specified with the front and the back. [Front form] and [Back form] can be chosen, respectively.
- | Double side overlay | Form data is printed on the surface specified by [Form data print face], and output data is printed on the other side of paper as variable data.
- | Single + Double side overlay | A form data and output data are printed on the surface and another form data is printed on the other side of paper.
Form data print face If [Double side overlay] is selected at [Form print pattern], set whether to print the form data onto the front side or the back side of paper. Specify Front and Back respectively When carrying out double-sided printing, different form can be specified and printed on the front side and the back side respectively. Form list The names of the data registered into the printer controller as "Form" is displayed. The form to print can be specified. Form Preview The selected form is previewed. Default Returns the settings on the [Forms] tab to the default settings. Help Displays Help.